# RS Feva Line Guide

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Description | Diameter | | Type | Length | Qty | |
| Halyards | | | | | | |
| Main Halyard | 4 | 5/32" | Eight Plait or Prestretch Polyester | 33' | 1 |
| Jib Halyard | 5 | 3/16" | Eight Plait or Prestretch Polyester | 22' | 1 | |
| Spinnaker Halyard | 4 | 5/32" | Eight Plait or Prestretch Polyester | 42' | 1 | |
| Sheets | | | | | | |
| Mainsheet | 5/16" | 8 mm | Doublebraid | 21' | 1 | |
| 2:1 Mainsheet | 5/16" | 8 mm | Doublebraid | 32' | 1 | |
| Jib Sheet | 1/4" | 6 mm | Doublebraid | 19' | 1 | |
| Spinnaker Sheet | 1/4" | 6 mm | Doublebraid | 27' | 1 | |
| Control Lines | | | | | | |
| Boomvang Cascade | 3/16" | 5 mm | Eight Plait or Prestretch Polyester | 7' | 1 | |
| Cunningham | 3/16" | 5 mm | Eight Plait or Prestretch Polyester | 3' 6" | 1 | |
| Outhaul | 3/16" | 5 mm | Eight Plait or Prestretch Polyester | 8' 6" | 1 | |
| Outhaul Take-Up | 3/16" | 5 mm | Shockcord | 8' | 1 | |
| Racing Outhaul | 5/32" | 4 mm | Eight Plait or Prestretch Polyester | 14' | 1 | |
| Other | | | | | | |
| Boomvang Boom Strop | 3/16" | 5 mm | Eight Plait or Prestretch Polyester | 1' 6" | 1 | |
| Boomvang Mast Strop | 3/16" | 5 mm | Eight Plait or Prestretch Polyester | 2' | 1 | |
| Daggerboard Handle | 5/16" | 8 mm | Doublebraid | 2' | 1 | |
| Daggerboard Retainer | 1/4" | 6 mm | Shockcord | 2' 6" | 1 | |
| Hiking Strap Elastic Front | 5/32" | 4 mm | Shockcord | 1' 6" | 2 | |
| Hiking Strap Elastic Rear | 3/16" | 5 mm | Shockcord | 3' 6" | 1 | |
| Hiking Strap Ties | 5/32" | 4 mm | Eight Plait or Prestretch Polyester | 1' 6" | 4 | |
| Jib Halyard Block Tie | 5/32" | 4 mm | Covered Spectra | 1' 6" | 1 | |
| Main Halyard Take-Up | 5/32" | 4 mm | Shockcord | 2' | 1 | |
| Mainsheet Bridle | 5/32" | 4 mm | Eight Plait or Prestretch Polyester | 6' | 1 | |
| Racing Outhaul Block Tie Down | 3/32" | 2 mm | Covered Spectra | 2' | 1 | |
| Righting Line | 3/16" | 5 mm | Eight Plait or Prestretch Polyester | 9' 6" | 2 | |
| Righting Line Take-up | 3/16" | 5 mm | Shockcord | 3' 6" | 2 | |
| Rudder Downhaul at Cleat | 5/32" | 4 mm | Eight Plait or Prestretch Polyester | 4' 6" | 1 | |
| Rudder Downhaul at Rudder | 5/32" | 4 mm | Covered Spectra | 2' | 1 | |
| Spinnaker Pole Launch Line | 5/32" | 4 mm | Eight Plait or Prestretch Polyester | 4' | 1 | |
| Spinnaker Pole Tack Line | 5/32" | 4 mm | Eight Plait or Prestretch Polyester | 8' | 1 | |
| Spinnaker Sheet Block Ties | 5/32" | 4 mm | Eight Plait or Prestretch Polyester | 1' | 2 | |
| Transom Carry Handles | 5/32" | 4 mm | Eight Plait or Prestretch Polyester | 2' | 2 | |